DC-D4532WERA
Architectural and Engineering Specifications

DC-D4532WERA
Architectural and Engineering Specifications
Version 1.2
[image: ]One Solution. One Company.

DC-D4532WERA
Architectural and Engineering Specifications


www.idisglobal.com | www.idis.co.kr
©2014 IDIS Co., Ltd. All rights reserved. IDIS and identifying product names and numbers herein are registered trademarks of IDIS Co., Ltd.
All non-IDIS brands and product names are trademarks of their respective companies.
Product appearance, build status and/or specifications are subject to change without notice.


[image: C:\Users\John.Chung\AppData\Local\Microsoft\Windows\INetCache\Content.Word\IDIS.PNG]6
Version 1.2

PART 1: PLEASE REFER TO ATTACHED DOCUMENTS - OVERVIEW & FORMAT SAMPLES
PART 2: PRODUCTS
Division 28 – Electric Safety and Security
Level 1 - 28.20.00 – Video Surveillance
Level 2 - 28.21.00 – Surveillance Cameras
Level 3 - 28.21.13 – IP Cameras
Manufacturer
1. IDIS Co., Ltd.
IDIS Tower, 344 Pangyo-ro, Bundang-gu
Seongnam-si, Gyeonggi-do, 13493, Korea
Tel: 	+82 31 723 5400
Fax: 	+82 31 723 5100
General
Product Description
The DC-D4532WERA is a 5-megapixel AI IR turret camera featuring IDIS LightMaster NIR technology. Designed for indoor and outdoor surveillance, the model is NDAA- and TAA-compliant and supports easy integration with IDIS DirectIP NVRs.
The camera delivers 2592 × 1944 resolution at 30 ips using a 1/2.8-inch progressive scan CMOS sensor. Its 3.2–10.5mm motorized varifocal lens provides remote focus and zoom, an F1.6–F3.3 aperture and P-Iris control. It supports 120dB True WDR, ICR day/night operation, H.265, H.264 (MP) and M-JPEG compression, IDIS Intelligent Codec and quadruple streaming. Minimum color illumination is 0.13 lux at F1.6. Additional imaging functions include de-fog and eight-zone privacy masking.
The IK10 vandal-resistant and IP67 weatherproof enclosure includes a heater. Six IR LEDs provide illumination up to 50 meters (164 ft). The operating temperature range is −40°C to +55°C, with startup at temperatures above −20°C.
IDIS Deep Learning Analytics (IDLA) supports object detection, intrusion, loitering, line crossing and face detection, with metadata for humans, vehicles and faces. Basic analytics include video motion detection and active tampering alarms.
Smart Failover supports microSD/SDHC/SDXC storage up to 512GB, complemented by a 60MB NLTSrec recording buffer. Connectivity includes ONVIF Profile S/T, one alarm input and one alarm output, and two-way audio with a built-in microphone, one line input and one line output. The camera also supports audio alarms. Power options are 12VDC (13.2W) and IEEE 802.3af Class 3 PoE (11.5W).

General Specification
1. The IP camera shall be equipped with 5 Megapixel 1/2.8” CMOS Sensor.
2. The IP camera shall be equipped with 3.2mm – 10.5mm motorized vari-focal lens, F1.6 – F3.3
3. The IP camera shall be a true day/night camera with a mechanical filter for low light performance.
The filter can be switched remotely, or automatically via a light level sensor or contact input (ICR).
4. The IP camera shall have wide dynamic range compensation (True WDR) for improved video quality in high-contrast situations (120 dB).
5. The IP camera shall be equipped with 6ea Infrared LED with range up to 50m (164ft).
6. The IP camera shall support P-Iris.
7. The IP camera shall utilize 2DNR/3DNR (Dynamic Noise Reduction) technology to reduce the bitrate and storage requirements by removing noise artifacts.
8. The IP camera shall be vandal proof and IP rating 67 complied dome enclosure design.
9. The IP camera shall be equipped with 10/100 Base-T, auto-sensing, half/full duplex, RJ-45 Ethernet connection.
10. The IP camera shall support industry standard Power over Ethernet (PoE) IEEE 802.3af, Class 3 to supply power to the camera over the network and 12VDC input.
11. The IP camera shall have built-in heater for continued use in subzero temperature conditions and utilize 12 VDC input to provide power.
12. The IP camera shall have on board microSD/SDHC/SDXC card backup storage slot as a safeguard against data loss during network interruptions.
13. Using IDIS NLTSrec(Non-Linear Time Shifting recording) technology, the IP camera can store the recording data to the internal recording memory buffer (60MB) in camera if there is a delay in data transmission due to the instantaneous load of the recorder or network, and then transmits the stored data to IDIS recorder safely.
14. The IP camera shall deliver maximum video resolution of 2592x1944 at rates up to 30ips (images per second).
15. The IP camera shall provide network connection using H.265, H.264(MP) and MJPEG compression. 
16. The IP camera shall support quadruple streams in DirectIP 2.0 protocol mode. 
17. The IP camera shall conform to the ONVIF Profile S/T.
18. The IP camera shall be equipped with embedded web server (IDIS Web) which works independently using a Web Browser with ActiveX plug-in.
19. The IP camera shall have Digest authentication, Password Protection, User access log, IP Filtering, IEEE802.1x(EAP-TLS), Chained Fingerprint, SSL Encryption and HTTPS Encryption for greater security.
20. The IP camera shall have network bandwidth limitation and MAT features for more efficient use of network bandwidth.
21. The IP camera shall have Easy network access via UPnP (Universal Plug and Play) function and embedded mDNS (Multicast DNS) protocol.
22. The IP camera shall have Intelligent Video Analysis (VA): 
· Object Metadata: Human, Vehicle, Face
· IDLA: Object Detection, Intrusion, Loitering, Line Crossing, Face Detection
· ETC: Video Motion Detection, Active Tampering Alarm

Protocol Specification: DirectIP 2.0
1.  The IP camera shall have DirectIP 2.0 mode. 
2.  DirectIP 2.0 protocol shall provide easy connection to DirectIP NVR for automatic discovery and video streaming configuration.
3.  DirectIP 2.0 shall provide the compatibility with IDIS Solution Suite VMS or ONVIF for third-party software solutions.
4.  DirectIP 2.0 shall support camera can be linked to IDIS software solution such as IDIS Center and IDIS Solution Suite, or 3rd party solution while it is being connected to a DirectIP NVR.
5.  DirectIP 2.0 camera shall be compatible with DirectIP 1.0 NVR as well as DirectIP 2.0 NVR.
6.  DirectIP 2.0 camera shall be unavailable for No-password login when connecting to DirectIP 2.0 NVR and IDIS Software Solutions.
7.  DirectIP 2.0 protocol shall provide Quadruple streams.
8.  DirectIP 2.0 protocol shall support H.264(MP) and H.265 and MJPEG compression.

Technical Specification
Video Specification
1. Image Sensor: 1/2.8” CMOS
2. Maximum Resolution: 2592 x 1944
3. Scanning Mode: Progressive Scan
4. Lens Type: Motorized Vari-focal (f=3.2–10.5mm, F1.6–F3.3)
5. Iris Control: P-Iris
6. Angular Field of View (H: Horizontal, V: Vertical, D: Diagonal):
[4:3 mode]
Wide : 98.9 º(H) 71.1º(V) 133.8 º(D) 
Tele : 28.2°(H) 21.2°(V) 35.3°(D) 
[16:9 mode]
Wide : 98.9°(H) 52.2°(V) 117.9°(D) 
Tele : 28.2°(H) 15.9°(V) 32.4°(D)

7. Pan/Tilt/Rotate Range : Pan: -180° ~ 180°, Tilt: -5° ~ 70°, Rotate: -180° ~ 180°
8. Minimum Illumination:
A. COLOR: 0.13 lux @ F1.6
B. B/W : 0 lux  (IR LED ON) 
9.   S/N Ratio: More than 45 dB
10. Maximum Frame Rate: 
A. 4:3 mode : 30ips : 2592 x 1944(WDR)
B. 16:9 mode : 30ips : 2592 x 1456(WDR)

11. Video Resolution:
A. 4:3 : 2592x1944, 1920x1440, 1280x960x 640x480
B. 16:9 : 2592x1456, 1920x1080, 1280x720, 640x360

12. Video Compression : H.265, H.264(MP), MJPEG
13. Video Compression Level: 4 levels: Basic, Standard, High, Very High
14. Intelligent Codec is supported.
15. Multi-Video Streaming: Quadruple streams
16. Dynamic Range: 120dB
17. True Day & Night: Yes (ICR)
18. IR Distance (The number of LEDs, IR wavelength): 50m (164ft) (6ea)
19. Intelligent Video Analytic: 
· Object Metadata: Human, Vehicle, Face
· IDLA: Object Detection, Intrusion, Loitering, Line Crossing, Face Detection
· ETC: Video Motion Detection, Active Tampering Alarm

Audio Specification
1. Audio Compression Algorithm: OPUS 16K, ADPCM 16K, G.726, G.711 u-Law, G.711 a-Law 
2. Audio Input / Output: 1(Built In MIC)+1 / 1
3. Two-way Audio Communication: Yes
4. Pre-recorded Voice Alert(Audio Alarm): Yes

Network Specification
1. Port: RJ-45 10/100 Base-T 1 port
2. Network Protocols: DirectIP 2.0 Protocol, IPv4, IPv6, RTP/RTSP/TCP, RTP/RTSP/HTTP/TCP,
RTP/UDP RTSP/TCP, HTTP, HTTPS, FTP, SNTP, SMTP, FEN, mDNS, uPNP, SNMPv2
3. Streaming Mode: Quadruple Streaming
Security Specification
1. [bookmark: _Hlk190700301]Digest authentication, Password Protection, User access log, IP Filtering, IEEE802.1x(EAP-TLS), Chained Fingerprint, SSL Encryption, HTTPS Encryption
2. Maximum Concurrent Session: 10 sessions shared across Admin, Watch, and Search, with a maximum of 1 Search session.
Alarm and Event Specification
1. Alarm Input / Output: 1 / 1
A. Alarm Input: TTL, NC/NO Programmable, 4.3V(NC) or 0.3V(NO) threshold, 5V DC
B. Mechanical or electrical switches can be wired to the Alarm-In and GND connectors. The maximum voltage should not exceed 5V.
C. Alarm Output: 1 TTL open collector, 30mA @ 5 VDC
2. Trigger Events: Motion Detection, Alarm in, Audio detection, Tampering, Object Detection, Intrusion, Loitering, Line Crossing, Face Detection
3. Event Notification: Remote S/W, Email (with Image)
A. Encryption Type: SSL
Environmental Specification
1. Operating Temperature: -40°C ~ +55°C (-40°F ~ +131°F)
*Starting up at above -20°C (-4°F)
2. Operating Humidity: 0% to 90% non-condensing
3. Vandal-proof Enclosure: IK10
4. Outdoor Ready: IP67, Heater
Electrical Specification
1. Power Source: 12VDC, PoE (IEEE 802.3af class 3)
2. Power Consumption: 
- 	PoE, IEEE 802.3af Class 3, 11.5W
- 	12V=, 1.1A, 13.2W
3. Regulatory Approvals: FCC, CE, KC
Mechanical Specification
1. Dimensions (Ø x H): Ø135 × 98.5mm
2. Unit Weight: 830g (1.83lb)
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